

--------------------------------------------------------------------------------------------------------------------------------

Burlap Panel Architectural Specifications CSI Sections 06, 09, 10

--------------------------------------------------------------------------------------------------------------------------------\*\* NOTE TO SPECIFIER \*\*: Homasote Company; floor and wall sound barrier.

.

This section is based on the products of Homasote Company, which is located at:

932 Lower Ferry Road

West Trenton, NJ 08628

Tel: (800) 257-9491

Tel: (609) 883-3300

Fax: (609) 883-3497

Email: sales@homasote.com

Web: http://www.homasote.com

Homasote 440 SoundBarrier® is controlling sound through millions of square feet of floors, walls and ceilings. a special-density, structural board made from 100 percent environmental Homasote® cellulose fiber, a homogeneous composition manufactured with uniformly distributed protection against termites, rot and fungi and resistance to moisture. It also insulates, with twice the R-value of wood.

An internationally known environmental icon, Homasote Company is the oldest manufacturer of building products made from recycled materials in the U.S., and the only manufacturer of its kind in the Americas.

Each production day Homasote Company recycles (and keep out of landfills) up to 100 tons of recycled paper. Every production year our unique manufacturing process helps conserve nearly 1.4 million trees and eliminates up to 65 million pounds of solid waste that otherwise would go into landfills.

Homasote Company’s environmental commitment extends beyond raw material recycling. It is the first manufacturer in the United States to recycle nearly all water used to manufacture its products. Process water, hundreds of thousands of gallons per day, is completely reused in a closed-loop system, a recycling feat recognized in 1956 by an award from the U.S. Army Corps of Engineers (precursor to the U.S. Environmental Protection Agency).

A leader in green building years before the first Earth Day was celebrated, Homasote Company naturally is a proud member of the U.S. Green Building Council. From sound control for floors and walls, to tackable interior panels, to roofing products, Homasote Company has a broad range of products with up to 98 percent recycled content that can help contribute towards LEED credits in several categories.

SECTION 09 80 00 - ACOUSTICAL TREATMENT

1. GENERAL
   1. SECTION INCLUDES

\*\* NOTE TO SPECIFIER \*\* Delete items below not required for project.

* + 1. Section 06 00 00 Wood, Plastics and Composites.
    2. Section 09 00 00 Finishes
    3. Section 10 00 00 Specialties
  1. RELATED SECTIONS

\*\* NOTE TO SPECIFIER \*\* Delete any sections below not relevant to this project; add others as required.

* + 1. Section 06 10 00 – Rough Carpentry: Installation and requirements for wood substrates and structure.
    2. Section 09 06 00 - Finishes.
    3. Section 09 20 00 – Plaster and Gypsum Board: Installation and requirements for wall assemblies.
  1. REFERENCES

\*\* NOTE TO SPECIFIER \*\* Delete references from the list below that are not actually required by the text of the edited section.

* + 1. Adhesive: meeting or exceeding APA AFG-01 specification.
    2. American Society for Testing and Materials (ASTM):
       1. ASTM C 209 - Test Methods for Cellulosic Fiber Insulating Board.
       2. ASTM C 518 - Standard Test Method for Steady-State Thermal Transmission Properties by Means of the Heat Flow Meter Apparatus.
       3. ASTM D 1037 - Test Methods of Evaluating Properties of Wood-Base Fiber and Particle Panel Materials.
       4. ASTM E 84 - Test Method for Surface Burning Characteristics of Building Materials.
       5. UL listed, File R16381.
       6. ICC-ES Report ESR-1374.
  1. SUBMITTALS
     1. Submit under provisions of Section 01 30 00.
     2. Product Data: Manufacturer's data sheets on each product to be used, including:
        1. Preparation instructions and recommendations.
        2. Storage and handling requirements and recommendations.
        3. Installation methods.
  2. QUALITY ASSURANCE
     1. Manufacturer Qualifications: Minimum 10 years experience in producing sound-deadening boards.
  3. DELIVERY, STORAGE, AND HANDLING
     1. Store products in manufacturer's unopened packaging with labels intact until ready for installation.
     2. Inspect the materials upon delivery to assure that specified products have been received. Report damaged material immediately to the delivering carrier and note such damage on the carrier's freight bill of lading.
     3. Store materials in a dry place, indoors, on raised platform protected from weather damage.
  4. PROJECT CONDITIONS
     1. Maintain environmental conditions (temperature, humidity, and ventilation) within limits recommended by manufacturer for optimum results. Do not install products under environmental conditions outside manufacturer's absolute limits.
     2. Acclimatize panels to existing moisture conditions and for not less than 24 hours before installation. Comply with manufacturer’s recommendations for acclimatization.

1. PRODUCTS
   1. MANUFACTURERS
      1. Acceptable Manufacturer: Homasote Company; 932 Lower Ferry Road, West Trenton, NJ 08628. Tel: (800) 257-9491. Tel: (609) 883-3300. Fax: (609) 883-3497. Email: sales@homasote.com. Website: www.homasote.com.
      2. Requests for substitutions will be considered in accordance with provisions of Section 01 60 00.

\*\* NOTE TO SPECIFIER \*\* Delete one of the following two paragraphs; coordinate with requirements of Division 1 section on product options and substitutions.

* + 1. Substitutions: Not permitted.
    2. Provide all finished acoustical wall panels from a single manufacturer.

\*\* NOTE TO SPECIFIER \*\* Consult manufacturer for specific recommendations of tested assembly constructions, STC ratings, and IIC ratings.

* 1. MATERIALS
     1. Homasote Burlap Panel: Class C fire-rated. Natural sustainable heavyweight jute fabric over 440 Homasote panel; a molded, recycled post-consumer paper, cellulose fiber structural panel. Physical properties as follows.

\*\* NOTE TO SPECIFIER \*\* Consult manufacturer for specific recommendations of tested assembly constructions, STC ratings, and IIC ratings. Delete thicknesses not required.

* + - 1. Thickness: 1/2 inch (13 mm).
      2. Density: 26-28 pcf (416-448 kg/cu. m) tested in accordance with ASTM C 209.
      3. Tensile Strength: When tested in accordance with ASTM C 209:
         1. Parallel: 450-700 psi (3,100-4,830 kPa).
         2. Transverse: 750-1000 psi (5.1171-6.894 kPa).
      4. Hardness (Janka Ball): 230 lbs (104 kg) tested in accordance with ASTM D 1037.
      5. Water Absorption by Volume: When tested in accordance with ASTM C 209:
         1. 2 hour immersion: 7 percent maximum.
      6. Expansion: 50 to 90 percent relative humidity, 0.25 percent in accordance with ASTM C 209.
      7. Thermal Resistance: When tested in accordance with ASTM C 209 per ASTM C 518:

\*\* NOTE TO SPECIFIER \*\* Consult manufacturer for specific recommendations of tested assembly constructions for required R-values. Delete thicknesses not required.

* + - * 1. R-value: 1.2 for 1/2 inch (13 mm) thick board.
      1. Noise reduction coefficient (NRC): 0.20
      2. Flame Spread: 76 to 200 tested in accordance with ASTM E 84, Class III or C.
    1. Edge detail: Burlap fabric wrapped along long edges only. 4’ ends are unwrapped.
  1. ACCESSORIES
     1. Metal Frame Clips: Manufacturer’s standard clip for securing panels to framing.

\*\* NOTE TO SPECIFIER \*\* Installation accessories are dependent on substrates and installation methods as recommended by the manufacturer; select from the following paragraphs accordingly.

* + 1. Adhesive: APA approved panel adhesive.
    2. Adhesive: APA AFG-01 subfloor adhesive.
    3. Wall Panel Fasteners:
       1. Nails: Color coordinated or decorative for paneling. Length required penetrating wood framing 3/4 inch (19 mm) minimum.
       2. Screws:
          1. General: 20 gauge or heavier, self-tapping drywall type steel screw.
          2. Wood Framing: Coarse thread drywall type wood screw, length as required to penetrate framing 3/4 inch (19 mm) minimum.
          3. Metal Framing: 22-25 gauge, drywall type steel screw.
          4. Decorative exposed fasteners determined by architect/specifier.

1. EXECUTION
   1. EXAMINATION
      1. Examine substrates upon which work will be installed.
      2. Verify framing member spacing complies with manufacturer’s requirements depending on substrates and installation methods.
      3. If substrate preparation is the responsibility of another installer, notify Architect of unsatisfactory preparation before proceeding.
      4. Verify what environmental conditions are, and will continue to be maintained in accordance with manufacturer’s recommendations.
      5. Starting work by installer is acceptance of substrate and environmental conditions.
   2. PREPARATION
      1. Follow manufacturer’s instructions by separating and allowing panels to be exposed to environmental temperature and humidity conditions for not less than 24 hours before start of installation.
      2. Temporarily position Burlap Panels in place and request architects’ approval, to ensure that desired appearance is obtained.
   3. INSTALLATION
      1. Install in accordance with manufacturer's instructions.
      2. Install only clean dry panels. Do not install wet panels.
      3. Refer to manufacturer’s installation instructions for proper procedures regarding the cutting and painting of the panel.
      4. Wall Panel Installation: Space panel joints 1/8 inch (3 mm) apart; 1/4 inch (6 mm) space at floors, ceilings, and window and door frames. Install gypsum wallboard or other wall finish panels first so that finish panel joints are staggered and do not coincide with Burlap Panel joints. Install in accordance with finish panel manufacturer’s installation recommendations.
   4. PROTECTION
      1. Protect installed products until completion of project.
      2. Touch-up, repair, or replace damaged products before Substantial Completion.
   5. CLEANING
      1. Comply with manufacturer's recommendations for panel cleaning procedures.
      2. Comply with manufacturer’s recommendations for repairing damaged panels.
      3. Replace panels that cannot be repaired.